|  |
| --- |
|  http://www.defib.ie/images/ce_mark.gif |
| CONDRON CONCRETE WORKS LTD14 |
| EN1916:2002225mm – 675mm DN**Unreinforced precast concrete pipe** for the conveyance of sewerage, rainwater and surface water, in pipelines that are generally buried.**Watertightness:** No leakage of joint or pipe at 50 kPa internally.**Crushing Strength:** Strength class 120.**Longitudinal bending strength:** Dimensionally adequate.**Durability:** Adequate for normal serviceability conditions.  |