|  |
| --- |
|  http://www.defib.ie/images/ce_mark.gif |
| CONDRON CONCRETE WORKS LTD14 |
| EN1917:2002Precast component for use in an inspection chamber.Reinforced concrete cover slab, corbel slab/adjusting unitWatertightness: No leakage of joint at 30 kPa internally.Mechanical resistance: Vertical strength 50 kN.Opening size: 600mm dia/600mm x 600mm/1200mm x 675mm.Durability: Adequate for normal serviceability conditions.  |